@ShortDescription

@ParamDescription(dely)
/* SoftClip Clip Threshold */
Threshold at which the saturation begins to be applied.

@ParamDescription(mbyp)
/* SoftClip Master Bypass */
Disables the saturation and passes the signal through untouched.

@Description
When the  the absolute value of the input signal level reaches the specified #param(dely) 
(on a sample by sample basis), Metric Halo Type 2 saturation is applied to the signal. 
Type 2 saturation is more aggressive than Type 1 saturation, but still provides relatively
gentle, low order distortion that is applied to the signal symmetrically.

The overall gain through the process block is automatically adjusted so that a full-scale 
input signal creates a full-scale output. When the input signal is below the specified 
#param(dely), the output signal is just the input signal with the over-all gain 
applied, and no additional non-linearity.

#name is useful for applying soft saturation in signal processing loops (for example, inside 
a feedback delay line). It is also useful for saturating the output of othe processors like the 
MIO Compressor and MIO Limiter.

@SeeAlso(MHL ,hcpM) /* MIOHardClipª */
@SeeAlso(MHL ,scp1) /* MIOSoftClip Type 1 */
@SeeAlso(MHL ,scp3) /* MIOSoftClip Type 3 */
