@ShortDescription

@ParamDescription(gain)
/*  Volume */
Specifies the gain applied to the input signal.

@ParamDescription(glid)
/*  Glide */
Specifies the rate at which the gain will change. If the Glide value is close to 0 (especially between .1 and 1), the gain will change slowly. If Glide is close to 1000, the gain will change quickly.

@ParamDescription(mbyp)
/*  Master Bypass */
When bypassed, the gain will be set to 0dB, passing the input signal unchanged.

@Description
The output of this plugin is the input with the specified gain applied to each input channel. The
gain is specifed by the #param(gain) parameter in dB. The #param(glid) parameter controls how quickly 
the applied gain will change when you change the #param(gain) parameter. This version of the plugin 
uses a single-pole low pass filter (LPF) to change the gain between the old value and the new value logarithmically. To change the gain linearly, use the #pi(MHL ,VLi2) plug-in.
