@ShortDescription
EnvelopeDetector — Envelope control signal extractor

@ParamDescription(attk)
/* Attack */
Controls how quickly the envelope follows the attack of the input signal.

@ParamDescription(rlse)
/* Release */
Controls how quickly the envelope follows the signal as the level drops below the current envelope level.

@ParamDescription(mbyp)
/* Master Bypass */
Has no effect on this plug-in.

@Description
#name is a mono process that generates the signal amplitude envelope from its input.
The output of #name may be used to apply the envelope of one signal to another or may be used as the control signal for any plug-in that supports control input. For example, it can be used to control the corner frequency of an #pi(MHL ,csvf) filter or the oscillation frequency of a #pi(MHL ,ncoQ). For these sorts of control inputs, you will generally need to map the range of the #name’s output to the range expected ny the control input. There are a variety of plug-ins in +DSP that can be used for this purpose, including #pi(MHL ,mmap) and #pi(MHL ,ncoT).

#name provides two parameters for controlling the envelope extraction process. #param(attk) controls how quickly the envelope follows the attack of the input signal and #param(rlse) controls how quickly the envelope follows the signal as the level drops below the current envelope level.
