@ShortDescription

@ParamDescription(dely)
/* Delay Delay(samp) */
Specifies the delay throught the process block in samples.

@ParamDescription(mbyp)
/* Delay Master Bypass */
When engaged sets the delay through the block to 0.

@Description
Provides an integer sample delay from the input to the output. Changes in the delay time 
are not interpolated, which means that changing the delay time will result in a glitch.
As a result, this delay is most suited for use as a fixed delay (as part of an algorithm or 
for a fixed compensation).

This version of the delay provides up to 255 samples of delay (5.3 ms @ 48k) and uses internal 
memory in the DSP to provide the highest possible DSP performance.


@SeeAlso(MHL ,DlyS) /* MIODelayª (s/s) */
@SeeAlso(MHL ,moDM) /* MIOModDelayª (m/m) */
@SeeAlso(MHL ,moDS) /* MIOModDelayª (s/s) */
@SeeAlso(MHL ,sDlM) /* MIO Delay (Short) (m/m) */
@SeeAlso(MHL ,sDlS) /* MIO Delay (Short) (s/s) */
@SeeAlso(MHL ,mDlM) /* MIO Delay (Medium) (m/m) */
@SeeAlso(MHL ,mDlS) /* MIO Delay (Medium) (s/s) */
@SeeAlso(MHL ,lDlM) /* MIO Delay (Long) (m/m) */
@SeeAlso(MHL ,lDlS) /* MIO Delay (Long) (s/s) */
@SeeAlso(MHL ,sDiM) /* MIO Delay (Short IM) (m/m) */
@SeeAlso(MHL ,sDiS) /* MIO Delay (Short IM) (s/s) */
@SeeAlso(MHL ,sMDM) /* MIO MultiTap Delay (Short) (m/m) */
@SeeAlso(MHL ,mMDM) /* MIO MultiTap Delay (Medium) (m/m) */
@SeeAlso(MHL ,lMDM) /* MIO MultiTap Delay (Long) (m/m) */
