@ShortDescription

@ParamDescription(dely)
/* Delay Delay(samp) */
Sets the maximum delay, in samples, applied to the input signal.

@ParamDescription(mbyp)
/* Delay Master Bypass */
When bypasssed, the delay through the process is 0.

@Description
#name is a dynamic, interpolating delay that uses a audio control signal to 
set the delay time through the process. The input control signal is clipped 
to the range of 0.0&hellip;1.0, and then is multipled with the maximum delay 
specified by #param(dely). The resulting fractional delay is applied to the 
input signal to form the output signal.

Since the delay is variable on a sample by sample basis, and it supports 
fractional delays, the #name can be used for automatic modulation effects 
like vibrato and chorus.

@SeeAlso(MHL ,DlyM) /* MIODelayª (m/m) */
@SeeAlso(MHL ,DlyS) /* MIODelayª (s/s) */
@SeeAlso(MHL ,moDS) /* MIOModDelayª (s/s) */
@SeeAlso(MHL ,sDlM) /* MIO Delay (Short) (m/m) */
@SeeAlso(MHL ,sDlS) /* MIO Delay (Short) (s/s) */
@SeeAlso(MHL ,mDlM) /* MIO Delay (Medium) (m/m) */
@SeeAlso(MHL ,mDlS) /* MIO Delay (Medium) (s/s) */
@SeeAlso(MHL ,lDlM) /* MIO Delay (Long) (m/m) */
@SeeAlso(MHL ,lDlS) /* MIO Delay (Long) (s/s) */
@SeeAlso(MHL ,sDiM) /* MIO Delay (Short IM) (m/m) */
@SeeAlso(MHL ,sDiS) /* MIO Delay (Short IM) (s/s) */
@SeeAlso(MHL ,sMDM) /* MIO MultiTap Delay (Short) (m/m) */
@SeeAlso(MHL ,mMDM) /* MIO MultiTap Delay (Medium) (m/m) */
@SeeAlso(MHL ,lMDM) /* MIO MultiTap Delay (Long) (m/m) */
