@ShortDescription

@ParamDescription(dely)
/* SoftClip Clip Threshold */
Threshold at which the saturation begins to be applied.

@ParamDescription(mbyp)
/* SoftClip Master Bypass */
Disables the saturation and passes the signal through untouched.

@Description
When the  the absolute value of the input signal level reaches the specified #param(dely) 
(on a sample by sample basis), Metric Halo Type 3 saturation is applied to the signal. 
Type 3 saturation is more aggressive than Type 2 saturation, and when driven sufficently
hard, can cause audible distortion, but is very useful in punching up percussive signals, and in 
softening rarely clipping signals.

The overall gain through the process block is automatically adjusted so that a full-scale 
input signal creates a full-scale output. When the input signal is below the specified 
#param(dely), the output signal is just the input signal with the over-all gain 
applied, and no additional non-linearity.

#name is useful for applying soft saturation in signal processing loops (for example, inside 
a feedback delay line). It is also useful for saturating the output of othe processors like the 
MIO Compressor and MIO Limiter.

@SeeAlso(MHL ,hcpM) /* MIOHardClipª */
@SeeAlso(MHL ,scp1) /* MIOSoftClip Type 1 */
@SeeAlso(MHL ,scp2) /* MIOSoftClip Type 2 */
