@ShortDescription

@Description
#name provides a Quadrature Oscillator whose oscillation frequency is controlled 
by the audio signal at the control input. The oscillation frequency changes 
approximately linearly with the input signal. 

The frequency of oscillation is 0 Hz when the control input is 1, and is Fs/2 when
the control input is -1.

@SeeAlso(MHL ,qudO) /* MIOQuadOscª */
@SeeAlso(MHL ,qLFO) /* MIOQuadLFOª */
@SeeAlso(MHL ,ncQG) /* MIOQuadNCO-Glide */
@SeeAlso(MHL ,nois) /* Noise */
