@ShortDescription

@ParamDescription(glid)
/* Osc Glide */
Sets the glide rate of the change of the oscillator frequency to changes in the control
signal input. When the Glide is set to 0, the 
oscillator will not change in response to changes in the control signal. 
When the glide is set to 1, the 
oscillator will change instantaneously (like the normal QuadNCO). 
In between values cause the oscillator to interpolate 
changes in the control signal at a faster or slower rate.

@Description
#name provides a Quadrature Oscillator whose oscillation frequency is controlled 
by the audio signal at the control input. The oscillation frequency changes 
approximately linearly with the input signal. 

The frequency of oscillation is 0 Hz when the control input is 1, and is Fs/2 when
the control input is -1.

#name filters the control input signal using the #param(glid) parameter to control how quickly
the oscillator frequency follows the control input.

@SeeAlso(MHL ,qudO) /* MIOQuadOscª */
@SeeAlso(MHL ,qLFO) /* MIOQuadLFOª */
@SeeAlso(MHL ,ncoQ) /* MIOQuadNCOª - Numerically Controlled Oscillator */
@SeeAlso(MHL ,nois) /* Noise */
