@ShortDescription

@ParamDescription(dely)
/* HardClip Clip Threshold */
Sets the linear sample value at which the input will be clipped.

@ParamDescription(mbyp)
/* HardClip Master Bypass */
Disables the clipper and passes the signal through untouched.

@Description
Applies a hard clipping threshold to the input signal. The #param(dely) specifies
the absolute level at which the signal will be clipped. If the absolute value of 
the signal (on a sample by sample basis) is greater than the level specified by #param(dely)
the output will be set to &plusmn; #param(dely) (with the sign determined by the sign of the
input sample).

This is equivalent to the hard clipping that occurs when a fixed point signal hits full-scale,
with the addition that you can adjust the level of the clipping point. This is not musically
useful by itself, but it is very useful in combination with other basic processing blocks.

@SeeAlso(MHL ,scp1) /* MIOSoftClip Type 1 */
@SeeAlso(MHL ,scp2) /* MIOSoftClip Type 2 */
@SeeAlso(MHL ,scp3) /* MIOSoftClip Type 3 */
