@ShortDescription
Convert Linear Control Signal to Control Signal for NCO

@ParamDescription(frqL)
/* Lo Freq */
sets the frequency generated by a connected NCO when the input control signal is 0.

@ParamDescription(frqH)
/* High Freq */
sets the frequency generated by a connected NCO when the input control signal is 1.

@Description
#name converts a control signal in the range [0, 1] to a control signal for the #pi(MHL ,ncoQ). 
You can specify the frequency that will be synthesized when the input control signal is 0 using the 
#param(frqL) parameter. Conversly, when the input control signal is 1, the synthesized frequency is
determined by the #param(frqH) parameter. The frequency genereated is linearly interpolated between
these the frequencies specified by the paramters for input signals between 0 and 1.If you set the 
#param(frqL) to be higher than the #param(frqH), the frequency synthesized will decrease as the 
input control signal increases.
