@ShortDescription
BandSplit – Crossover for Mobile I/O

@ParamDescription(freq)
/* F */
Sets the crossover frequency (in Hz) of the bandsplit.

@Description
#name is a mono in, two out crossover module. The input is processed by a 24dB/octave Linkwitz-Riley filter, with frequencies below #param(freq) output from the “Low” output and those above #param(freq) output from the “High” output.

@SeeAlso(MHL ,bsps) /* Band Split (s) */