@ShortDescription

@ParamDescription(dely)
/* SoftClip Clip Threshold */
Threshold at which the saturation begins to be applied.

@ParamDescription(mbyp)
/* SoftClip Master Bypass */
Disables the distortion generator and causes the output to be zero.

@Description
When the  the absolute value of the input signal level reaches the specified #param(dely) 
(on a sample by sample basis), Metric Halo Type 3 distortion is generated and sent to the 
output. This signal may be added to the input to generate the same effect the Type 3 soft
clipper. The point of this signal processing module is to allow you to further process the 
distortion signal before adding it back into the original signal.

@SeeAlso(MHL ,sdt1) /* MIOSoftDistortion Type 1 */
@SeeAlso(MHL ,sdt2) /* MIOSoftDistortion Type 2 */
