@ShortDescription

@ParamDescription(eqen)
/*  Enable */
Enables the EQ block. When disabled, the EQ (including the master gain) is hard-bypassed,
and does not consume DSP power.

@ParamDescription(emgn)
/*  Gain */
Master gain applied to the signal at the output of the EQ block. Since the EQ is implemented
as a high-resolution floating point process, you can bring the output signal of the EQ out of 
any degree of clipping using this parameter.

/************************************************************************************/
@ParamDescription(eqe1)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg1)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf1)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb1)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt1)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqe2)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg2)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf2)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb2)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt2)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqe3)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg3)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf3)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb3)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt3)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqe4)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg4)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf4)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb4)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt4)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqe5)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg5)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf5)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb5)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt5)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqe6)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg6)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf6)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb6)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt6)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqe7)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg7)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf7)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb7)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt7)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqe8)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg8)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf8)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb8)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt8)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqe9)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqg9)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqf9)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqb9)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqt9)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqeA)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqgA)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqfA)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqbA)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqtA)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqeB)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqgB)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqfB)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqbB)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqtB)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

/************************************************************************************/
@ParamDescription(eqeC)
/*  Band 1 Enable */
Enables the band. When disabled, the band is hard-bypassed.

@ParamDescription(eqgC)
/*  Band 1 Gain */
Sets the parameteric gain on the EQ band. For peaking filters, this is the gain at the peak of 
the band. For shelving filters, this is the gain at the extreme limit of the filter. This 
parameter is ignored for the high and low pass filter types as well as the bandpass filter type.

@ParamDescription(eqfC)
/*  Band 1 Frequency */
Sets the characteristic frequency of the filter band.

@ParamDescription(eqbC)
/*  Band 1 Bandwidth */
Sets the bandwidth of the filter band in octaves.

@ParamDescription(eqtC)
/*  Band 1 Type */
Chooses the type of filter that is applied for the band.

@ParamDescription(mbyp)
/*  Master Bypass */
Disables the EQ block. When disabled, the EQ (including the master gain) is hard-bypassed,
and does not consume DSP power.

@Description
#name implements a mono 6-band IIR EQ processor. Each band is fully parameteric, and can be set 
to any of the filter types. All the parameters of all the bands can be set to any of valid settings.
The composite EQ curve is applied to the input signal, and the master gain is then applied to the 
processed signal. 

<indexterm><primary>RIAA decoder</primary></indexterm>Note: Each band of EQ is capable of being configured as one of 6 types of EQ Filter. The types are: 
Peaking/Parametric, Low Shelf, Hi Shelf, Hi Cut, Low Cut, Band Pass, and RIAA. The first 5 types are 
parametric filters that allow you to use the Frequency, Gain and Bandwidth controls to adjust position
and shape of the filter that is applied. The RIAA type is special. It is used to decode a signal 
that has been RIAA encoded (for example, the signal on a phonograph disc). This filter type would be 
selected if you need to decode the output of a phonograph player that is directly connected to the 
inputs of your interface, with the use of an external RIAA phono preamp. Only one band of EQ should 
be set to RIAA on a channel as using the filter twice will not provide useful results.


@SeeAlso(MHL ,eq6S) /* MIOEqª 6 Band (s/s) */
@SeeAlso(MHL ,eqcM) /* MIOEqª 12 Band (m/m) */
@SeeAlso(MHL ,eqcS) /* MIOEqª 12 Band (s/s) */
