@ShortDescription
Scale and Offset Signal

@ParamDescription(scal)
/* ScaleOffset Scale */
Gain applied to input signal.

@ParamDescription(offs)
/* ScaleOffset Offset */
DC-Offset added to the scaled input signal.

@ParamDescription(mbyp)
/* ScaleOffset Master Bypass */
When engaged, the process block is hard-bypassed, and the output signal
is the same as the input signal.

@Description
#name is used to apply an affine transformation to the input signal on a 
sample by sample basis. This can be used to suitably scale and offset control
signals used as audio-rate controls for blocks that accept such signals, or it can be 
used to set scale and bias on signals before they are driven into non-linear elements.
The added DC bias can be used to condition the waveshaping applied by the nonlinear
signalprocessing blocks. The remaining DC offset can be removed by another #name instance, or by
using a DC-Block filter.

