@ShortDescription

@ParamDescription(minv)
/* Main Mid Invert */
When enabled, inverts the 1st input channel before processing.

@ParamDescription(sinv)
/* Main Side Invert */
When enabled, inverts the 2nd input channel before processing.

@ParamDescription(wdth)
/* Main Width */
Adjusts the width of the transformed field. When this parameter is 0, the ouput will be
mono. When this is 1, the full stereo width is represented.

@ParamDescription(mbyp)
/* Main Master Bypass */
Bypasses all of the processing.

@Description
#name is a Mid/Side Decoder. It can be used to decode material that 
was previously encoded as Mid/Side.
