@ShortDescription

@ParamDescription(step)
/* Osc Steps */
Sets the amount of pitch-shift applied to the input in half-steps. This parameter
supports micro-tonal shifts. 

@Description
The #name is a monophonic process block that shifts the pitch of the input signal
by the specified number of half-steps (12 half-steps per octave). 

The #name provides one parameter (#param(step)), which is the amount of pitch 
shift to apply to the signal. The shift parameter has a range of -24 half-steps
(-2 Octaves) to +24 half-steps (+2 Octaves), and may take on any fractional
value in the range. 

There is a small amount of effective delay on the pitch shifted signal, but it
is generally not noticable when the shifted signal is summed back with the original
signal. Depending upon the frequency of the input signal there may be a small amount
of AM modulation in the output signal. This will appear as apparent tremolo on the output.
